|  |  |
| --- | --- |
| Title | MarchInn 12V DC 3.0T(6600lb) Electric Hydraulic Floor Jack and Tire Inflator Pump and LED Flashlight 3 in 1 Set with Electric Impact Wrench Car Repair Tool Kit |
| Bullet points |  POWERFUL: Work with 12V vehicle power outlet, 3.0T(6600lb) jack capacity and 340N.M powerful torque.   EFFICIENT: Lift the car in less than a minute by the jack, remove the screws by the wrench, change a tire quickly.   CONVENIENT: The design of the jack is succinct and easy to operate with compact and organized storage box.   MUTILFUCTION: Jack, pump, wrench and can meet multiple demands. Essential tool for outdoor emergency.   SAFE: The structure is stable and secure. Machine will stop working when it lifts beyond the height limit. |
| Description | **The MarchInn 12V DC Automatic Electric Car Repair Tool Kit is worth having for emergency roadside tire change and repair. 2 sleeves with 4 size of 17mm,19mm,21mm,23mm, suitable for most of vehicle. Cross groove saddle prevent slipping from vehicle. Rotating threaded rod can be spin out up to 75mm, makes cross groove saddle closer to lifting point. In case of the power has been disconnected, self-locking power structure and safety unloading knob prevent jack from falling and will not come down immediately. When re-connecting the power, jack will go on working in accordance with the instruction, or using the safety valve manually to fall. LED lamp on jack can be used as flashlight.**  **Specification:** a. For Electric Jack: Input Voltage: 12V DC Max Current: 13A Rated Power: 150W Max Loading: 6600lb (3.0T) Lifting Height Range: 6.1 in. -17.7 in. (155mm-450mm)  Power Cord Length: 11.5 ft. (3.5m)  b. For Electric Inflator Pump: Air Flow: 9.2 gal/min (35 L/min) Max Pressure: 10 BAR/150 PSI Hose Length: 25.6 in. (0.65m)  c. For Electric Impact Wrench: Input Voltage: 12V DC Max Current: 12A Rated Power: 100W Max. Torque: 340N.M Cable Lengh: 3.5 M(11.5 Feet)  **Packing List:** Combo 2 in 1 Electric Hydraulic Jack: 1 pc Electric Impact Wrench: 1 pc Safety Hammer: 1 pc Plastic Tool Box: 1 pc Double-sided lug nut sockets: 2 pcs (23mm( 7/8" ) 21mm(13/16") 19mm (3/4") 17mm( 11/16" )) Power Cable: 1 pc 10 Feet in Length Battery Clamp Connecting Cable: 1 pc Fuses: 2 pcs Gloves: 1 pair Reflective safety Triangle to warn on coming Motorists Instruciton Manual: 2 pcs (One is for jack, the other is for wrench)  **Warning:** Please read this manual carefully before using. |

