|  |  |
| --- | --- |
| Title | MarchInn Electric Car Scissor Jack for 12V DC 3.0T（6600lb） |
| Bullet points |  POWERFUL: Work with 12V vehicle power outlet, 3.0T(6600lb) jack capacity.   EFFICIENT: Lift the car in less than one minute, and change a tire quickly.   CONVENIENT: The design of the jack is succinct and easy to operate with compact and organized storage box.   DURABLE: The body is made of high-strength steel, not easily deformed.   SAFE: The structure is stable and secure. Machine will stop working when it lifts beyond the height limit. |
| Description | **The MarchInn 12 Volt Automatic Electric Car Jack is worth having for emergency roadside tire change and repair.  The reinforced solid screw rod and high-strength steel body makes it strong and durable. And it’s also anti-rust and wear resistant because of the whole anti-oxidation painting body.  It’s energy saving due to the 12 V DC low power motor.Battery clips with 12 V DC could be used to connect battery if car cigarette lighter is inoperative.  The quadrilateral base and cross groove saddle makes it stable and reliable. It’s totally water-proof so you can use it even on rainy day.**  **Specification:** Input Voltage: 12V DC Max Current: 15A Rated Power: 120W Max Loading: 6600 lb (3000 kg) Lifting Height Range: 4.7 in. -17.7 in. (120mm-450mm)  Power Cord Length: 11.5 ft. (3.5m) Jack Weight: 11 lbs(4.99kg)  **Packing List:** Electric Car Jack: 1 pc Plug for car cigarette lighter (3.5m):1 pc Plug for car battery:1 pc Spare fuse(12A): 3 pcs Double-sided lug nut sockets : 2 pcs (23mm( 7/8" ) 21mm(13/16") 19mm (3/4") 17mm( 11/16" )) Wheel nut wrench:1pc Gloves: 1 pair Crank handle:1 pc  **Warning:** Please read the manual carefully before using.   **One year warranty, if the product you purchase is broken within one year, we will resend the parts or even the whole one.** |

